#include <Metriful_sensor.h>

// How often to read and report the data (every 3, 100 or 300 seconds)
#define CYCLE_PERIOD = CYCLE_PERIOD_3_S

// The details of the WiFi network:
#define WIFI_SSID = "..." // network SSID (name, case sensitive)
#define WIFI_PASSWORD = "..." // network password

// Home Assistant settings

// You must have already installed Home Assistant on a computer on your 
// network. Go to www.home-assistant.io for help on this.

// Choose a unique name for this MS430 sensor board so you can identify it.
// Variables in HA will have names like: SENSOR_NAME.temperature, etc.
#define SENSOR_NAME "metriful_living_room"

// Change this to the IP address of the computer running Home Assistant. 
// You can find this from the admin interface of your router.
#define HOME_ASSISTANT_IP "..."

// Security access token: the Readme and User Guide explain how to get this
#define LONG_LIVED_ACCESS_TOKEN "..."
